{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"merged":[[0,0,0,5],[17,0,18,0],[17,1,18,1],[20,0,22,0],[20,1,22,1],[23,0,25,0],[23,1,25,1],[41,0,44,0],[41,1,44,1],[50,0,50,2],[50,3,50,5],[51,0,51,2],[51,3,51,5],[52,0,52,5],[53,0,53,5]],"flags":["formulas_cached_only"]}
["2025年度零星基建维修工程项目\n报价单"]
["序号","项目内容","项目特征描述","单位","含税单价","备注"]
[1,"更换井盖","铸铁材料","个"]
[2,"更换井盖","水泥材料","个"]
[3,"更换门锁",null,"个"]
[4,"磁吸门帘透明挡风隔热门帘",null,"㎡"]
[5,"换玻璃(含拆，装)","不足1平方按1平方结算","㎡"]
[6,"贴玻璃纸","不足1平方按1平方结算","㎡"]
[7,"水管漏水处理",null,"点"]
[8,"更换球阀","Φ32以下(含32)","个"]
[9,"更换球阀","Φ40以上(含40)","个"]
[10,"OA地板铺设","同通士达已铺设OA地板铺设","㎡"]
[11,"OA地板维修","修补地面板","㎡"]
[12,"维修卷闸门",null,"次"]
[13,"管道疏通（主管道）",null,"个"]
[14,"管道疏通（分管道）",null,"个"]
[15,"管道疏通（分管道）","一次三个（含）以上","个"]
[16,"施工零星砌筑工程","多孔砖墙;工程部位：地上、下内外墙\n1.砖品种、规格、强度等级:190厚水泥多孔砖，强度等级MU10\n2.砂浆强度等级、配合比:M5混合砂浆","m³\n"]
[null,null,"砖墙;工程部位：地上、下内外墙\n1.砖品种、规格、强度等级:120厚砖，强度等级MU10\n2.砂浆强度等级、配合比:M5混合砂浆","m³\n"]
[17,"施工水泥砂浆粉刷（含底层、面层及抹平）","墙面一般抹灰；1、9厚1:3水泥砂浆底层，2、6厚1:2.5水泥砂浆抹平压光","m²"]
[18,"施工地面、道路混凝土施工工程"," 垫层,1.混凝土种类:非泵送商品混凝土2.混凝土强度等级:C15\n2.混凝土强度等级:C15 ","m³\n"]
[null,null," 道路地面[碎石 C20]非 商品混凝土，混凝土强度等级:C20 ","m³\n"]
[null,null," 2cm水泥砂浆楼地面面层（抹光）","m²"]
[19,"施工门、窗制作、安装工程","不锈钢门，材质:304型号（含五金配件、门锁、闭门器等）","m²"]
[null,null,"方管400*400、镀锌钢板门（镀锌板单面，含五金配件、门锁）3*3.5米","m²"]
[null,null," 铝合金推拉窗制作,铝铝合金门","m²"]
[20," 楼地面装饰施工工程"," 施工地面钢砖600*600含结合层水泥砂浆","m²"]
[21,"施工地面钢砖"," 施工地面钢砖800*800含结合层结构胶","m²"]
[22,"施工地面花岗岩","石材楼地面 平台；1、25厚花岗石板饰面，\n2、30厚1:3干硬性水泥砂浆粘结层\n","m²"]
[23,"施工墙、柱面装饰与隔断、幕墙铁件工程","工字钢，槽钢，角钢；钢结构（钢结构屋架，平台，楼梯，等加固件）制作，安装","吨"]
[24,"施工彩钢板、方管支架、围挡制作、安装","彩钢板、30*30cm方管支架、围挡制作、安装（施工）","m²"]
[25,"施工轻钢龙骨隔墙","双面石膏板隔墙，含轻钢龙骨及配件，安装","m²"]
[26,"施工轻钢龙骨隔墙","双面硅酸钙板隔墙，含轻钢龙骨及配件，安装","m²"]
[27,"施工彩钢岩棉夹芯板（型号426、填充岩棉）","1.轻质隔热彩钢夹芯板墙 (墙厚50mm)\n2、含包角、包边、配件、安装费用、损耗","m²"]
[28,"施工墙面、天棚乳胶漆涂料项目"," 墙面、天棚面修补、乳胶漆涂料","m²"]
[29,"施工安装铝塑板吊顶含配件","铝塑板规格600*600、600*300mm","m²"]
[30,"维修铝塑板吊顶含配件","铝塑板规格600*600、600*300mm","m²"]
[31,"维修彩钢板夹心板、钢结构配件、门、隔墙","含人工电焊、切割、配件、安装。不含彩钢板夹心板、钢结构配件主材","m²"]
[32,"维修不锈钢材料吊顶","不锈钢门吊顶，材质:304型号（含五金配件、损耗等）","m²"]
[33,"维修石膏板吊顶","石膏板吊顶维修、更换600*600含材料，配件、损耗","m²"]
[34,"施工金属结构施工油漆","金属结构刷油漆；底漆一遍，面漆二遍，含除锈1.除锈级别:轻锈\n2.油漆品种:红丹防锈漆、调和漆\n3.结构类型:一般钢结构\n","m²"]
[35,"维修、零星拆除工程","人工拆除塑料门窗项目","m²"]
[null,null,"人工拆除彩钢岩棉夹芯板","m²"]
[null,null,"人工拆除钢砖（花岗岩）地面及结合层、厚25cm","m²"]
[null,null,"人工拆除钢结构件（含彩钢板）屋面、墙面项目","m²"]
[36,"人工切割、拆除混凝土地面","拆除地面混凝土、切割、风爆打100mm混凝土基层（水泥砂浆结合层）200mm","m³\n"]
[37,"切割水磨地面（裂缝、空洞）混凝土及水泥砂浆修补地面","1、切割水磨地面（裂缝、空洞）、混凝土。2、高标号水泥砂浆修补地面","m²"]
[38,"土头外运至规定收纳点","人工装卸、土头外运、汽车装运容量4m3/车","车"]
[39,"措施满堂脚手架","装修满堂脚手架 基本层3.5m-5.2m","m²"]
[40,"措施钢管脚手架","外墙扣件式钢管脚手架 双排 建筑物高度30m以内","m²"]
["单价合计"]
["税率"]
["1.以上报价为工料费以及土头垃圾清运出厂区的费用，均为含税报价\n2.本工程所需材料均由投标人提供，由投标人自行采购、运输、保管。\n3.应急抢修项目投标人应于接到通知后24小时内做出实质性响应（人员、工具、设备等到达指定地点）。\n4.该基建维修一般工程项目的质量保修期12个月，其余建筑项目质量保修期按有关规定执行。"]
["投标人：（签字盖章）\n日期："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}